;************************************************************************
;FILENAME: se091010mgmt.inf
;Copyright Sony Ericsson Mobile Communications AB/LTD/INC 2009. All rights reserved.
;
;The program(s) may be used and/or copied only with the written permission
;from Sony Ericsson Mobile Communications AB or in accordance with the terms
;and conditions stipulated in the agreement/contract under which the
;program(s) have been supplied.
;************************************************************************ 

[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%SEMC%
DriverVer=05/13/2009,1.0.3.1  ; Date format: MM/DD/YYYY
CatalogFile=se091010mgmt.cat

[Manufacturer]
%SEMC% = Models, NTia64, NTamd64

[Models]
%INTERFACE1% = Install, %MODEL_HARDWARE_ID1%
%INTERFACE2% = Install, %MODEL_HARDWARE_ID2%
%INTERFACE3% = Install, %MODEL_HARDWARE_ID3%

[Models.NTia64]
%INTERFACE1% = Install, %MODEL_HARDWARE_ID1%
%INTERFACE2% = Install, %MODEL_HARDWARE_ID2%
%INTERFACE3% = Install, %MODEL_HARDWARE_ID3%

[Models.NTamd64]
%INTERFACE1% = Install, %MODEL_HARDWARE_ID1%
%INTERFACE2% = Install, %MODEL_HARDWARE_ID2%
%INTERFACE3% = Install, %MODEL_HARDWARE_ID3%

[Install.NT]
CopyINF=se091010mdm.inf, se091010mtp.inf
AddReg=Install.NT.AddReg
Include = mdmcpq.inf
CopyFiles=FakeModemCopyFileSection

[Install.NT.Services]
AddService = usbser, 0x00000002, Services

[Install.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[Services]
DisplayName = %SERIAL%
Description	= %SERIAL%
ServiceType = 1
StartType = 3
ErrorControl = 0
ServiceBinary = %12%\usbser.sys
LoadOrderGroup = Base

[Strings]
SEMC = "Sony Ericsson Mobile Communications AB"
INTERFACE1 = "Sony Ericsson Device 091010 USB Serial Port"
INTERFACE2 = "Sony Ericsson Device 091010 USB OBEX Port"
INTERFACE3 = "Sony Ericsson Device 091010 USB Application Port"
SERIAL = "Sony Ericsson USB Serial Port"
MODEL_HARDWARE_ID1 = "USB\VID_0FCE&PID_D10E&MI_01" ; SP1 - SERIAL
MODEL_HARDWARE_ID2 = "USB\VID_0FCE&PID_D10E&MI_05" ; SP2 - OBEX
MODEL_HARDWARE_ID3 = "USB\VID_0FCE&PID_D10E&MI_07" ; SP3 - APPLICATION

[SourceDisksNames]
; none

[SourceDisksFiles]
; none
