;-------------------------------------------------------------------------------
; Novatel Wireless Merlin UMTS Modem
; Installation file (.inf).
; (c) Copyright 2003 Novatel Wireless Inc.
;-------------------------------------------------------------------------------
;
;when          who   what, where, why
;-----------   ---   -----------------------------------------------------------
;11 Nov 2004   HT    Changed child HW ID to generic
;12 Sep 2004   HT    UMTS 630 HW ID
;13 Jul 2004   HT    384Kbps Update & SkipEnumerations
;17 Dec 2003   HT    Changed to Serial Port device
;-------------------------------------------------------------------------------

;-------------------------------------------------------------------------------
; INF Version Section
;-------------------------------------------------------------------------------
[version]
signature="$CHICAGO$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider       = %nwProvider%
CatalogFile.NT = NwtUMTS.cat
CatalogFile.NTAMD64 = NwtUMTS64.cat
DriverVer      = 11/26/2006,1.3.5.4

;-------------------------------------------------------------------------------
; INF Manufactuerer Section
;-------------------------------------------------------------------------------
[Manufacturer]
%nwProvider%=Nwt,NTamd64

;-------------------------------------------------------------------------------
; INF Models Section
;-------------------------------------------------------------------------------
[Nwt]
%mf\novatel_wireless-merlin_umts_modem-dev1.DeviceDesc% = Ports, mf\novatel_wireless-merlin_umts_modem-dev1 ; Communications Port

[Nwt.NTamd64]
%mf\novatel_wireless-merlin_umts_modem-dev1.DeviceDesc% = Ports, mf\novatel_wireless-merlin_umts_modem-dev1 ; Communications Port

;-------------------------------------------------------------------------------
; INF DDInstall Section
;-------------------------------------------------------------------------------
[Ports.NT]
AddReg=Ports.AddReg, Ports.NT.AddReg
LogConfig=c14,c1a,c23,c2a,c34,c3a,c43,c4a,caa

[Ports.NTamd64]
AddReg=Ports.AddReg, Ports.NT.AddReg
LogConfig=c14,c1a,c23,c2a,c34,c3a,c43,c4a,caa

[Ports.AddReg]
HKR,,PortSubClass,1,01

[Ports.NT.AddReg]
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
; Uncomment the following line if you want to override the advanced dialog for
; your device.  See msports.h for protoype of OverrideAdvancedFunction
; HKR,,EnumAdvancedDialog,,"yourdll.dll,OverrideAdvancedFunction"

;-------------------------------------------------------------------------------
; INF DDInstall.HW Section
;-------------------------------------------------------------------------------
[Ports.NT.HW]
AddReg=Ports.NT.HW.AddReg

[Ports.NTamd64.HW]
AddReg=Ports.NT.HW.AddReg

[Ports.NT.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"serenum"
HKR,,SkipEnumerations,0x00010001,0xFFFFFFFF
HKR,,"EnablePowerManagement",0x00010001, 1

;-------------------------------------------------------------------------------
; INF DDInstall.Services Section
;-------------------------------------------------------------------------------
[Ports.NT.Services]
Include=msports.inf
Needs=ComPort.NT.Services

[Ports.NTamd64.Services]
Include=msports.inf
Needs=ComPort.NT.Services

;-------------------------------------------------------------------------------
; INF Novatel defines Section
;-------------------------------------------------------------------------------

; The following sections are COM port resource configs.
; Section name format means:
; Char 1 = c (COM port)
; Char 2 = I/O config: 1 (3f8), 2 (2f8), 3 (3e8), 4 (2e8), a (any)
; Char 3 = IRQ config: #, a (any)

[c14]                   ; COM1,IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=4

[c1a]                   ; COM1, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=3,4,5,7,9,10,11,12,14,15

[c23]                   ; COM2, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=3

[c2a]                   ; COM2, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=3,4,5,7,9,10,11,12,14,15

[c34]                   ; COM3, IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=4

[c3a]                   ; COM3, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=3,4,5,7,9,10,11,12,14,15

[c43]                   ; COM4, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=3,5

[c4a]                   ; COM4, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=3,4,5,7,9,10,11,12,14,15

[caa]                   ; Any base, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=8@100-ffff%fff8(3ff::)
IRQConfig=3,4,5,7,9,10,11,12,14,15

; End COM port LogConfig sections


;-------------------------------------------------------------------------------
; INF Strings Section
;-------------------------------------------------------------------------------
[Strings]
nwProvider     = "Novatel Wireless Inc"
mf\novatel_wireless-merlin_umts_modem-d022_dev1.DeviceDesc = "Novatel Wireless UMTS Modem Secondary Port"
mf\novatel_wireless-merlin_umts_modem-dev1-29e4.DeviceDesc = "Novatel Wireless UMTS Modem Secondary Port"
mf\novatel_wireless-merlin_umts_modem-dev1.DeviceDesc = "Novatel Wireless UMTS Modem Secondary Port"
NWSrcDisk      = "Novatel Wireless Driver Disk"
