; Windows Modem Setup File
; Manufacturer: Sony Ericsson Mobile Communications
; Copyright (c) 2007 Sony Ericsson Mobile Communications AB
;-----------------------------------------------------------------------------------

[Version]
Signature="$WINDOWS NT$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%SEM%
DriverVer=05/24/2007, 1.1
Catalogfile=SEM125.cat

[Controlflags]
ExcludeFromSelect=*

[DestinationDirs]
MSIRCOMM.CopyFiles=12
DefaultDestDir=12

[Manufacturer]
%SEM% = SEM,NTamd64

[SEM]
%Modem% = Modem,IRENUM\SERB026
%Modem% = Modem,IRENUM\SERB029
%Modem% = Modem,IRENUM\SERB032
%Modem% = Modem,IRENUM\SERB040
%Modem% = Modem,IRENUM\SERB041
%Modem% = Modem,IRENUM\SERB042
%Modem% = Modem,IRENUM\SERB053
%Modem% = Modem,IRENUM\SERB057
%Modem% = Modem,IRENUM\SERB072
%Modem% = Modem,IRENUM\SERB090
%Modem% = Modem,IRENUM\SERB0A2

[SEM.NTamd64]
%Modem% = Modem,IRENUM\SERB026
%Modem% = Modem,IRENUM\SERB029
%Modem% = Modem,IRENUM\SERB032
%Modem% = Modem,IRENUM\SERB040
%Modem% = Modem,IRENUM\SERB041
%Modem% = Modem,IRENUM\SERB042
%Modem% = Modem,IRENUM\SERB053
%Modem% = Modem,IRENUM\SERB057
%Modem% = Modem,IRENUM\SERB072
%Modem% = Modem,IRENUM\SERB090
%Modem% = Modem,IRENUM\SERB0A2

[Modem.NT]
include=MDMIRMDM.inf
needs=MDMIRMDM.MSIRCOMM.CopyFiles
AddReg=All, Addreg, Responses, External

[Modem.NT.Services]
include=MDMIRMDM.inf
needs=MDMIRMDM.MSIRCOMM.AddService

[Modem.NT.HW]
include=MDMIRMDM.inf
needs=MDMIRMDM.MSIRCOMM.LowerFilterAddReg

[All]
HKR,,ConfigDialog,,modemui.dll
HKR,,PortSubClass,1,02
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"

[External]
HKR,, DeviceType, 1, 01

[Addreg]
HKR,,ConfigDelay, 1, A0,0F,00,00
HKR,, DeviceType, 1, 01

HKR,, Properties, 1, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 30,00,00,00, 00,C2,01,00, 80,70,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,C2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR, Settings, CompatibilityFlags, 1, 01 ,00 ,00, 00

HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 2,, "None"
HKR, Hangup, 1,, "ATH<cr>"
HKR, Answer, 1,, "ATA<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Init,1,, "AT<cr>"
HKR, Init,2,, "AT &F<cr>"
HKR, Init,3,, "AT V1E0S0=0&D2&C1<cr>"
HKR, Init,4,, "AT +CMEE=1;+CVHU=1<cr>"

HKR, Settings, FlowControl_Hard,, "+IFC=2,2;"
HKR, Settings, FlowControl_Off,,  "+IFC=0,0;"
HKR, Settings, FlowControl_Soft,, "+IFC=1,1;"
HKR, Settings, Compression_On,, "+DS=3,0,2048,32;"
HKR, Settings, Compression_Off,, "+DS=0;"
HKR, Settings, CallSetupFailTimer,, "S7=<#>;"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, InactivityTimeout,, ""
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"

[Responses]
HKR, Responses, "0<cr>",    1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK - Command executed
HKR, Responses, "1<cr>",    1, 02, 00, 00,00,00,00, 00,00,00,00 ; CONNECT - Connection
HKR, Responses, "2<cr>",    1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING - Ring signal indicated
HKR, Responses, "3<cr>",    1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER 
HKR, Responses, "4<cr>",    1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR - Invalid command
HKR, Responses, "5<cr>",    1, 02, 00, B0,04,00,00, 00,00,00,00 ; CONNECT 1200
HKR, Responses, "6<cr>",    1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE - No dial tone detected
HKR, Responses, "7<cr>",    1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY - Engaged (busy) signal
HKR, Responses, "8<cr>",    1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER

HKR, Responses, "<cr><lf>OK<cr><lf>",                     1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",                   1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",             1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",                  1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>",            1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIAL TONE<cr><lf>",           1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",                   1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",              1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",                1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",           1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",           1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",           1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>",          1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",          1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800<cr><lf>",          1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600<cr><lf>",          1, 02, 00, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",          1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",          1, 02, 00, 00,e1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",         1, 02, 00, 00,c2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>FAX<cr><lf>",                    1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATA<cr><lf>",                   1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>VOICE<cr><lf>",                  1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RINGING<cr><lf>",                1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DELAYED<cr><lf>",                1, 1D, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DELAYED NUMBER<cr><lf>",         1, 1D, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BLACKLISTED<cr><lf>",            1, 1C, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BLACKLISTED NUMBER<cr><lf>",     1, 1C, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+FCERROR<cr><lf>",               1, 03, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>+CME ERROR: 0<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Phone failure.
HKR, Responses, "<cr><lf>+CME ERROR: 1<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; No connection to phone.
HKR, Responses, "<cr><lf>+CME ERROR: 2<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Phone modem link reserved.
HKR, Responses, "<cr><lf>+CME ERROR: 3<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Operation not permitted.
HKR, Responses, "<cr><lf>+CME ERROR: 4<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; Operation not supported.
HKR, Responses, "<cr><lf>+CME ERROR: 5<cr><lf>",    1, 03, 00, 00,00,00,00, 00,00,00,00   ; PH-SIM card PIN required.
HKR, Responses, "<cr><lf>+CME ERROR: 10<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card not inserted.
HKR, Responses, "<cr><lf>+CME ERROR: 11<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card PIN required.
HKR, Responses, "<cr><lf>+CME ERROR: 12<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card PUK required.
HKR, Responses, "<cr><lf>+CME ERROR: 13<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card failure.
HKR, Responses, "<cr><lf>+CME ERROR: 14<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card busy.
HKR, Responses, "<cr><lf>+CME ERROR: 15<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; SIM card wrong.
HKR, Responses, "<cr><lf>+CME ERROR: 16<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Incorrect password.
HKR, Responses, "<cr><lf>+CME ERROR: 20<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Memory full.
HKR, Responses, "<cr><lf>+CME ERROR: 21<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Invalid index.
HKR, Responses, "<cr><lf>+CME ERROR: 22<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Not found.
HKR, Responses, "<cr><lf>+CME ERROR: 23<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Memory failure.
HKR, Responses, "<cr><lf>+CME ERROR: 24<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Text string too long.
HKR, Responses, "<cr><lf>+CME ERROR: 25<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Invalid character in text string.
HKR, Responses, "<cr><lf>+CME ERROR: 26<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Dial string too long.
HKR, Responses, "<cr><lf>+CME ERROR: 27<cr><lf>",   1, 03, 00, 00,00,00,00, 00,00,00,00   ; Invalid character in dial string.
HKR, Responses, "<cr><lf>+CME ERROR: 100<cr><lf>",  1, 03, 00, 00,00,00,00, 00,00,00,00   ; Unknown.
HKR, Responses, "<cr><lf>+CMS ERROR: ",             1, 03, 00, 00,00,00,00, 00,00,00,00   ; CMS errors

[Strings]
SEM	= "Sony Ericsson Mobile Communications"
Modem  = "Sony Ericsson IrDA Modem 125"
