;
;  Purpose:   Netcard setup information file for Windows 95(OSR2) / 98(SE) / ME / 2000 / XP
;
;  Author:    Tevin Chen
;
;  Date:      Apr, 2003
;
;  Copyright: ZyXEL Communications Corporation
;

[Version]
CatalogFile = getndis.cat
Signature   = "$Chicago$"
Compatible  = 1
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Prov%
DriverVer   = 04/22/2003, 1.11.0.0069

[Manufacturer]
%Manuf%     = MANUF

[MANUF]
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_3302187E
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119

;-------------------------------------------------------------------------------
; ndi for 3119
;-------------------------------------------------------------------------------
[VT3119.ndi]
DelReg          = GET.delreg
AddReg          = VT3119.reg, GET.reg, FlowCtrl.reg, GET.reg.win, Tagging.reg, VLAN.reg, Jumbo.reg
CopyFiles       = GET.ndi.CopyFiles

[VT3119.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = GET.delreg
AddReg          = VT3119.reg, GET.reg, FlowCtrl.reg, GET.reg.NT, Tagging.reg, VLAN.reg, RxCksmOfld.reg.NT, TxTaskOfld.reg.NT, Jumbo.reg
CopyFiles       = GET.CopyFiles.NT

[VT3119.ndi.NT.Services]
AddService      = GETNDIS, 2, GET.Service, GET.EventLog

;-------------------------------------------------------------------------------
; VT3119 specific , AdapterCFID = 0x31191106 (HEX) = 823726342 (DEC)
;
[VT3119.reg]
HKR, Ndi,                           DeviceID,       0, "PCI\VEN_1106&DEV_3119"
HKR, ,                              AdapterCFID,    0, "823726342"
HKR, ,                              AdapterType,    0, "5"
HKR, ,                              MediaType,      0, "1"

HKR, ,                              ReceiveBurstIndicate,   0, "64"
HKR, ,                              ReceiveThreshold,       0, "0"
HKR, ,                              BurstLength,            0, "7"
HKR, ,                              MapRegisters,           0, "128"
HKR, ,                              EarlyReceive,           0, "0"
HKR, ,                              EarlyTransmit,          0, "0"
HKR, ,                              TxSupThr,               0, "31"
HKR, ,                              RxSupThr,               0, "7"
HKR, ,                              TCPLSSeg,               0, "8"
HKR, ,                              SyncTIC,                0, "1"

HKR, ,                              TransmitBuffers, 0, "128"
HKR, Ndi\params\TransmitBuffers,    ParamDesc,       0, %TXBuffer%
HKR, Ndi\params\TransmitBuffers,    default,         0, "128"
HKR, Ndi\params\TransmitBuffers,    type,            0, "int"
HKR, Ndi\params\TransmitBuffers,    Min,             0, "64"
HKR, Ndi\params\TransmitBuffers,    Max,             0, "256"
HKR, Ndi\params\TransmitBuffers,    Step,            0, "1"
HKR, Ndi\params\TransmitBuffers,    Base,            0, "10"
HKR, Ndi\params\TransmitBuffers,    flag,            1, "20","00","00","00"

HKR, ,                              ReceiveBuffers,  0, "128"
HKR, Ndi\params\ReceiveBuffers,     ParamDesc,       0, %RXBuffer%
HKR, Ndi\params\ReceiveBuffers,     default,         0, "128"
HKR, Ndi\params\ReceiveBuffers,     type,            0, "int"
HKR, Ndi\params\ReceiveBuffers,     Min,             0, "64"
HKR, Ndi\params\ReceiveBuffers,     Max,             0, "256"
HKR, Ndi\params\ReceiveBuffers,     Step,            0, "1"
HKR, Ndi\params\ReceiveBuffers,     Base,            0, "10"
HKR, Ndi\params\ReceiveBuffers,     flag,            1, "20","00","00","00"

; Nway Forced Mode
HKR, ,                              NwayForce,       0, "1"

; Power Management Capability
HKR, ,                              PMC,             0, "0"

;-------------------------------------------------------------------------------
; GET common driver parameters
;
[GET.reg]

; Connection Type
HKR, ,                                      ConnectionType, 0, "0"
HKR, Ndi\params\ConnectionType,             ParamDesc,      0, %ConnectionType%
HKR, Ndi\params\ConnectionType,             default,        0, "0"
HKR, Ndi\params\ConnectionType,             type,           0, "enum"
HKR, Ndi\params\ConnectionType\enum,        0,              0, %autoN%
HKR, Ndi\params\ConnectionType\enum,        1,              0, %100HD%
HKR, Ndi\params\ConnectionType\enum,        2,              0, %100FD%
HKR, Ndi\params\ConnectionType\enum,        3,              0, %10HD%
HKR, Ndi\params\ConnectionType\enum,        4,              0, %10FD%
HKR, Ndi\params\ConnectionType,             flag,           1, "30","00","00","00"

; User defined Network Address
HKR, ,                                      NetworkAddress, 0, ""
HKR, Ndi\params\NetworkAddress,             ParamDesc,      0, %NetAddress%
HKR, Ndi\params\NetworkAddress,             Default,        0, ""
HKR, Ndi\params\NetworkAddress,             type,           0, "edit"
HKR, NDI\params\NetworkAddress,             LimitText,      0, "12"
HKR, NDI\params\NetworkAddress,             UpperCase,      0, "1"
HKR, NDI\params\NetworkAddress,             optional,       0, "1"
HKR, NDI\params\NetworkAddress,             Base,           0, "16"
HKR, Ndi\params\NetworkAddress,             flag,           1, "20","00","00","00"

; Validate Rx SNAP/802.3 packet length
HKR, ,                                      ValidatePacketLen, 0, "0"

[FlowCtrl.reg]
; Flow control capability advertisement
HKR, ,                                      FlowCtrl,       0, "0"
HKR, Ndi\params\FlowCtrl,                   ParamDesc,      0, %FlowCtl%
HKR, Ndi\params\FlowCtrl,                   default,        0, "0"
HKR, Ndi\params\FlowCtrl,                   type,           0, "enum"
HKR, Ndi\params\FlowCtrl\enum,              0,              0, %HwDefault%
HKR, Ndi\params\FlowCtrl\enum,              1,              0, %EnableTx%
HKR, Ndi\params\FlowCtrl\enum,              2,              0, %EnableRx%
HKR, Ndi\params\FlowCtrl\enum,              3,              0, %EnableTxRx%
HKR, Ndi\params\FlowCtrl\enum,              4,              0, %Disabled%
HKR, Ndi\params\FlowCtrl,                   flag,           1, "20","00","00","00"

[GET.reg.win]
; Win95/Win98/WinME
HKR, Ndi,                                   NdiInstaller,   0, "wndi.dll,NdiProc"
HKR, Ndi\Install,                           ndis3,          0, "GET.ndis5"

HKR, NDIS,                                  MajorNdisVersion,1,03
HKR, NDIS,                                  MinorNdisVersion,1,0A
HKR, ,                                      DevLoader,      0, "*ndis"
HKR, ,                                      DeviceVxDs,     0, "getnd5a.sys"
HKR, NDIS,                                  LogDriverName,  0, "GETNDIS"

HKR, Ndi\Interfaces,                        DefLower,       0, "ethernet"
HKR, Ndi\Interfaces,                        LowerRange,     0, "ethernet"
HKR, Ndi\Interfaces,                        DefUpper,       0, "ndis3,ndis2"
HKR, Ndi\Interfaces,                        UpperRange,     0, "ndis3"

; the parameter below are in windows 95(OSR2)/98(SE)/ME only
; Wake On LAN Event
HKR, ,                                      WOLEvent,       0, "0"
HKR, Ndi\params\WOLEvent,                   ParamDesc,      0, %WOLEvent%
HKR, Ndi\params\WOLEvent,                   default,        0, "0"
HKR, Ndi\params\WOLEvent,                   type,           0, "enum"
HKR, Ndi\params\WOLEvent\enum,              0,              0, %OSDefault%
HKR, Ndi\params\WOLEvent\enum,              1,              0, %OSAndUnicast%
HKR, Ndi\params\WOLEvent,                   flag,           1, "20","00","00","00"

[Tagging.reg]
; number of Tx queue allocation
HKR, ,                                      TxQueueNum,     0, "4"
; 802.1p/802.1q Packet Tagging
HKR, ,                                      8021pqtag,      0, "0"
HKR,Ndi\Params\8021pqtag,                   ParamDesc,      0, %8021pq%
HKR,Ndi\Params\8021pqtag,                   Default,        0, "0"
HKR,Ndi\Params\8021pqtag,                   type,           0, "enum"
HKR,Ndi\Params\8021pqtag\enum,              "0",            0, %Disabled%
HKR,Ndi\Params\8021pqtag\enum,              "1",            0, %Enabled%
HKR,Ndi\params\8021pqtag,                   flag,           1, "20","00","00","00"

[VLAN.reg]
; static single VLAN ID setting
HKR, ,                                      VLANID,         0, "0"
HKR, Ndi\params\VLANID,                     ParamDesc,      0, %VLANID%
HKR, Ndi\params\VLANID,                     default,        0, "0"
HKR, Ndi\params\VLANID,                     type,           0, "int"
HKR, Ndi\params\VLANID,                     Min,            0, "0"
HKR, Ndi\params\VLANID,                     Max,            0, "4094"
HKR, Ndi\params\VLANID,                     Step,           0, "1"
HKR, Ndi\params\VLANID,                     Base,           0, "10"
HKR, Ndi\params\VLANID,                     flag,           1, "20","00","00","00"

[GET.reg.NT]
; Windows 2000/XP
HKR, Ndi\Interfaces,                        LowerRange,     0, "ethernet"
HKR, Ndi\Interfaces,                        UpperRange,     0, "ndis5"
HKR, Ndi,                                   Service,        0, "GETNDIS"
; ScatterGather DMA Capability -> Optimized for performance
HKR, ,                                      ScatterGather,  0, "1"
HKR, Ndi\params\ScatterGather,              ParamDesc,      0, %Optimized%
HKR, Ndi\params\ScatterGather,              default,        0, "1"
HKR, Ndi\params\ScatterGather,              type,           0, "enum"
HKR, Ndi\params\ScatterGather\enum,         0,              0, %Disabled%
HKR, Ndi\params\ScatterGather\enum,         1,              0, %Enabled%
HKR, Ndi\params\ScatterGather,              flag,           1, "20","00","00","00"

[RxCksmOfld.reg.NT]
HKR, ,                                     RxCksmOfld,      0, "0"
HKR, Ndi\params\RxCksmOfld,                ParamDesc,       0, %RxCksmOfld%
HKR, Ndi\params\RxCksmOfld,                default,         0, "0"
HKR, Ndi\params\RxCksmOfld,                type,            0, "enum"
HKR, Ndi\params\RxCksmOfld\enum,           0,               0, %Disabled%
HKR, Ndi\params\RxCksmOfld\enum,           1,               0, %Enabled%
HKR, Ndi\params\RxCksmOfld,                flag,            1, "20","00","00","00"

[TxTaskOfld.reg.NT]
HKR, ,                                     TxTaskOfld,      0, "2"
HKR, Ndi\params\TxTaskOfld,                ParamDesc,       0, %TxTaskOfld%
HKR, Ndi\params\TxTaskOfld,                default,         0, "2"
HKR, Ndi\params\TxTaskOfld,                type,            0, "enum"
HKR, Ndi\params\TxTaskOfld\enum,           0,               0, %Disabled%
HKR, Ndi\params\TxTaskOfld\enum,           1,               0, %TxTaskOfldCksm%
HKR, Ndi\params\TxTaskOfld\enum,           2,               0, %TxTaskOfldTcpLS%
HKR, Ndi\params\TxTaskOfld,                flag,            1, "20","00","00","00"

[Jumbo.reg]
HKR, ,                                      Jumbo,          0, "0"
HKR, Ndi\params\Jumbo,                      ParamDesc,      0, %Jumbo%
HKR, Ndi\params\Jumbo,                      default,        0, "0"
HKR, Ndi\params\Jumbo,                      type,           0, "enum"
HKR, Ndi\params\Jumbo\enum,                 0,              0, %Disabled%
HKR, Ndi\params\Jumbo\enum,                 1,              0, %Enabled%
HKR, Ndi\params\Jumbo,                      flag,           1, "20","00","00","00"

;-------------------------------------------------------------------------------
; Installation for NT
;

[GET.CopyFiles.NT]
getnd5b.sys,,,2

[GET.Service]
DisplayName     = %GET.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\getnd5b.sys
LoadOrderGroup  = NDIS

[GET.EventLog]
AddReg = GET.AddEventLog.reg

[GET.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;-------------------------------------------------------------------------------
; Installation for Windows 95/98/ME
;

[GET.ndis5]
CopyFiles=GET.ndis5.CopyFiles

[GET.ndis4]
CopyFiles=GET.ndis4.CopyFiles

[GET.ndis3]
CopyFiles=GET.ndis3.CopyFiles

;-------------------------------------------------------------------------------
; CopyFiles sections for Windows 95/98/ME
;

[GET.ndi.CopyFiles]
wndi.dll,,,2

[GET.ndis5.CopyFiles]
getnd5a.sys,,,2

[GET.ndis4.CopyFiles]
getnd4.sys,,,2

[GET.ndis3.CopyFiles]
getnd3.sys,,,2

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir          = 11
GET.CopyFiles.NT        = 12

[SourceDisksFiles]
getnd5a.sys         = 1
getnd5b.sys         = 1
getnd4.sys          = 1
getnd3.sys          = 1
getndis.inf         = 1
wndi.dll            = 1

[SourceDisksNames]
1 = %DiskName%,,,

;-------------------------------------------------------------------------------
; Uninstall/DelFiles/DelReg
;
[GET.delreg]
HKR,Ndi\Params

;-------------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
Prov                = "ZyXEL Communications Corporation"
DiskName            = "Network Adapter source disk"
ConnectionType      = "Connection Type"
autoN               = "Auto-Negotiation"
100HD               = "100BaseTx Half Duplex"
100FD               = "100BaseTx Full Duplex"
10HD                = "10BaseT   Half Duplex"
10FD                = "10BaseT   Full Duplex"
Disabled            = "Disabled"
Enabled             = "Enabled"
WOLEvent            = "Wake On LAN Event"
OSDefault           = "OS Default Event"
OSAndUnicast        = "OS Default & Unicast"
TXBuffer            = "Transmit Buffers"
RXBuffer            = "Receive Buffers"
NetAddress          = "Network Address"
FlowCtl             = "Flow Control"
HwDefault           = "Hardware Default"
EnableTx            = "Enable Tx"
EnableRx            = "Enable Rx"
EnableTxRx          = "Enable Tx/Rx"
8021pq              = "802.1p/Q Tagging"
VLANID              = "VLAN ID"
RxCksmOfld          = "Rx Checksum Offload"
TxTaskOfld          = "Tx Task Offload"
TxTaskOfldCksm      = "Checksum Offload"
TxTaskOfldTcpLS     = "Checksum and TCP Large Send Offload"
Optimized           = "Optimized for performance"
Jumbo               = "Jumbo Frames Support"

Manuf   = "ZyXEL Communications Corporation"
VT3119.DeviceDesc    = "ZyXEL OMNI LAN PCI G1 1000Base-T Adapter"
GET.Service.DispName = "ZyXEL OMNI LAN PCI G1 1000Base-T Adapter Driver"
