;*****************************************************************************
;
; Name:  zebrscep.inf
;
; Function:
;	Install the Sony Ericsson PC-Connect Port VCOMM drivers (Ports class)
;
; Copyright (c) 2007 MCCI Corporation
;
; MCCI is a registered trademark of MCCI Corporation.
; 
; NOTICE: This software is licensed, not sold.  Any modification of this
; inf file to change the reference to an operating system or to change the
; reference to a device is not permitted unless authorized in writing by
; MCCI Corporation.
;
;*****************************************************************************

[Version]
signature="$WINDOWS NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%Provider%
DriverVer=12/26/2007,4.40.6.0
CatalogFile=zebrsce.cat


[ControlFlags]
ExcludeFromSelect = *

[SourceDisksNames.x86]
; diskid = description[, [tagfile] [, <unused>, subdir]]
1=%DiskString%,"zebrsce.sys",,\i386

[SourceDisksNames.amd64]
; diskid = description[, [tagfile] [, <unused>, subdir]]
1=%DiskString%,"zebrsce.sys",,\amd64

[SourceDisksFiles]
; filename = diskid[,[ subdir][, size]]
zebrsce.sys = 1
zebrcmnt.sys = 1

;-----------------------------------------------------------------------------
; Specify target paths...
;-----------------------------------------------------------------------------

[DestinationDirs]
DefaultDestDir = 12                    ; system32\drivers

;-----------------------------------------------------------------------------
; Table of Contents
;-----------------------------------------------------------------------------
[Manufacturer]
%SEMC%=SEMC, NTamd64

;-----------------------------------------------------------------------------
; Device-by-device entries
;-----------------------------------------------------------------------------
[SEMC]
%SEMC.SCE_Comm.Desc% = SEMC.Install, MCCICEB\CEB_zebrceb&SCE_{8164CCDF-8A85-48c4-9A2D-5D9735DAF48E}&OS_NT
%PortDesc% = SEMC.Install, ZEBRCR\{8A572185-9558-41e2-BA5C-5E00C9E46F48}

[SEMC.NTamd64]
%SEMC.SCE_Comm.Desc% = SEMC.Install, MCCICEB\CEB_zebrceb&SCE_{8164CCDF-8A85-48c4-9A2D-5D9735DAF48E}&OS_NT
%PortDesc% = SEMC.Install, ZEBRCR\{8A572185-9558-41e2-BA5C-5E00C9E46F48}

;-----------------------------------------------------------------------------
;       How to install the upper VXD driver on W95/W98
;-----------------------------------------------------------------------------
[SEMC.Install]
AddReg		= SEMC.W95AddReg,SEMC.W95Overrides
[SEMC.Install.Hw]
AddReg = SEMC.mRouter

[SEMC.mRouter]
HKR,,"mRouter",0x00010001,1


;-----------------------------------------------------------------------------
;       How to install the WDM driver on NT
;-----------------------------------------------------------------------------
[SEMC.Install.nt]
AddReg		= SEMC.AddReg,SEMC.NT.AddReg
CopyFiles	= CopyFiles, CopyFiles.Win2K


;-----------------------------------------------------------------------------
;  Registry
;-----------------------------------------------------------------------------

; common registry entries 
[SEMC.AddReg]
HKR,,NTMPDriver,,zebrsce.sys
HKR,,EnableCR1146, 0x10001, 01,00,00,00 
HKR,,InitialBaudRate, 0x10001, 00,C2,01,00			;115200 initial baud rate
HKR,,InitialLineControl,, "8N1"					;8-bits, No parity, 1 stop bit

;**** here's the stuff for W95 ports.
;**** it's in this INF file, but we'll not use it until we get enumerated.
[SEMC.W95AddReg]
HKR,,DevLoader,,*vcomm
HKR,,PortDriver,,zebrcomm.vxd
HKR,,Contention,,zebrvcd.vxd
HKR,,DCB,3,1C,00,00,00, 00,C2,01,00, 11,33,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,PortSubClass,1,01
HKR,,ConfigDialog,,serialui.dll
HKR,,EnumPropPages,,"serialui.dll,EnumPropPages"

;-----------------------------------------------------------------------------
;  Logical Configurations
;-----------------------------------------------------------------------------
[SEMC.W95Overrides]
;-- Config for 3f8 - COM1,IRQ4
HKR,Override,0000,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
F8,03,FF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
10,00,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 2f8 0 COM2 IRQ3
HKR,Override,0001,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
F8,02,FF,02, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
08,00,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 3e8 0 COM3 IRQ4
HKR,Override,0002,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
E8,03,EF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
10,00,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 2e8 0 COM4 IRQ3
HKR,Override,0003,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
E8,02,EF,02, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
08,00,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;-- Config for 3f8 - COM1 IRQAny
HKR,Override,0004,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
F8,03,FF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 2f8 0 COM2 IRQAny
HKR,Override,0005,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
F8,02,FF,02, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 3e8 0 COM3 IRQAny
HKR,Override,0006,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
E8,03,EF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 2e8 0 COM4 IRQAny
HKR,Override,0007,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
E8,02,EF,02, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for anywhere- COMx IRQ Any
HKR,Override,0008,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
00,01,FF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for anywhere- COMx IRQ None
HKR,Override,0009,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
00,01,FF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** TERMINATOR ***
00,00,00,00

; only for NT...
[SEMC.NT.AddReg]
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

;-----------------------------------------------------------------------------
;  Copy lists
;-----------------------------------------------------------------------------
[CopyFiles]

[CopyFiles.Win2K]
zebrsce.sys
zebrcm.sys,zebrcmnt.sys
zebrcmnt.sys


;-----------------------------------------------------------------------------
;  NT Services installation
;-----------------------------------------------------------------------------
[SEMC.Install.NT.HW]
AddReg = LowerFilterAddReg

[SEMC.Install.NT.Services]
AddService = zebrsce, 0x00000002, SEMC.Install.AddService



[SEMC.Install.AddService]
DisplayName	= %SEMC.Service.Name%
Description	= %SEMC.Service.Desc%
ServiceType	= 1			;%SERVICE_KERNEL_DRIVER%
StartType	= 3			;%SERVICE_DEMAND_START%
ErrorControl	= 1			;%SERVICE_ERROR_NORMAL%	
ServiceBinary	= %12%\zebrsce.sys



[LowerFilterAddReg]
HKR,,"mRouter",0x00010001,1

;-----------------------------------------------------------------------------
; STRINGS
;-----------------------------------------------------------------------------
[Strings]

;<<localize the following>>

;BEGIN ENG - US English Strings

Provider = "Sony Ericsson Mobile Communications AB"
SEMC = "Sony Ericsson Mobile Communications AB"
DiskString = "Sony Ericsson PC-Connect Port Installation Disk"

PortDesc = "Sony Ericsson PC-Connect Port (VCOMM)"

SEMC.SCE_Comm.Desc = "Sony Ericsson PC-Connect Port"
SEMC.Service.Name = "Sony Ericsson PC-Connect Port"
SEMC.Service.Desc = "Sony Ericsson PC-Connect Port"


CustomerDataPath = "Sony Ericsson"
DriverSet = "Sony Ericsson Symbian 9 Drivers"
UninstallFile = "ZEBRUninstall.exe"
McciOptions = "Uninstallable"

;END ENG - US English Strings

;-----------------------------------------------------------------------------
; The following are symbolic constants which don't change per locale.
;-----------------------------------------------------------------------------


;*** end of file ***
