;****************************************************************************************
;
; rt2870.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Ralink RT2870 series USB Wireless LAN Card.
;
;   Copyright (c)2007 , Ralink Technology Corp., All Rights Reserved
;   All Rights Reserved.
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Ralink%
Compatible      = 1
DriverVer       = 07/28/2007, 1.00.04.0000
CatalogFile     = rt2870.cat            ;for WHQL certified

[ControlFlags]
;***********Ralink 802.11 n board  ***********
;ExcludeFromSelect = USB\VID_148F&PID_2870

[Manufacturer]
%Ralink%        = Ralink
%Asus%          = ASUS
%Sitecom%       = Sitecom
%Conceptronic%  = Conceptronic
%Planex%        = Planex
%D-Link%        = D-Link
%AL%            = AL
%Airlink%       = Airlink
%Corega%        = Corega
%Gigabyte%      = Gigabyte
%Sparklan%      = Sparklan
%SMC%           = SMC
%Arcadyan%      = Arcadyan
%ZCOM%          = ZCOM
%EnGenius%      = EnGenius
%Philips%       = Philips
%Draytek%       = Draytek
%AzureWave%     = AzureWave

[Ralink]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Generic.DeviceDesc%        = Ralink.ndi,           USB\VID_148F&PID_2870
%Generic.DeviceDesc%        = Ralink_2770.ndi,      USB\VID_148F&PID_2770

[ASUS]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ASUS.DeviceDesc%           = ASUS.ndi,             USB\VID_0B05&PID_1731
%ASUSGEN.DeviceDesc%        = ASUSGEN.ndi,          USB\VID_0B05&PID_1732
%ASUS1742.DeviceDesc%       = ASUS1742.ndi,         USB\VID_0B05&PID_1742

[Sitecom]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sitecom.DeviceDesc%        = Sitecom.ndi,          USB\VID_0DF6&PID_0017

[Conceptronic]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Conceptronic.DeviceDesc%   = Conceptronic.ndi,     USB\VID_14B2&PID_3C06

[Planex]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Planex.DeviceDesc%         = Planex.ndi,           USB\VID_2019&PID_ED06

[D-Link]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%D-Link.DeviceDesc%         = D-Link.ndi,           USB\VID_07D1&PID_3C09

[AL]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AL.DeviceDesc%             = AL.ndi,               USB\VID_14B2&PID_3C07

[Airlink]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Airlink.DeviceDesc%        = Airlink.ndi,          USB\VID_14B2&PID_3C23

[Corega]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Corega.DeviceDesc%         = Corega.ndi,           USB\VID_07AA&PID_002F

[Gigabyte]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Gigabyte.DeviceDesc%       = Gigabyte.ndi,         USB\VID_1044&PID_800B

[Sparklan]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sparklan.DeviceDesc%       = Sparklan.ndi,         USB\VID_15A9&PID_0006

[SMC]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%SMC.DeviceDesc%            = SMC.ndi,              USB\VID_083A&PID_B522

[Arcadyan]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Arcadyan.DeviceDesc%       = Arcadyan.ndi,         USB\VID_083A&PID_7522

[ZCOM]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ZCOM.DeviceDesc%           = ZCOM.ndi,             USB\VID_0CDE&PID_0022

[EnGenius]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%EnGenius.DeviceDesc%       = EnGenius.ndi,         USB\VID_1740&PID_9701

[Philips]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Philips.DeviceDesc%        = Philips.ndi,          USB\VID_0471&PID_200F

[Draytek]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Draytek.DeviceDesc%        = Draytek.ndi,          USB\VID_14B2&PID_3C25

[AzureWave]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AzureWave.DeviceDesc%      = AzureWave.ndi,        USB\VID_13D3&PID_3247

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[Ralink.ndi]
AddReg                  = USB_148F_2870.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Ralink_2770.ndi]
AddReg                  = USB_148F_2770.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[ASUS.ndi]
AddReg                  = USB_0B05_1731.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[ASUSGEN.ndi]
AddReg                  = USB_0B05_1732.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[ASUS1742.ndi]
AddReg                  = USB_0B05_1742.ndi.reg, Common.reg, USB9X.ndi.reg, RemoveFlag.reg
CopyFiles               = win9x.CopyFiles

[Sitecom.ndi]
AddReg                  = USB_0DF6_0017.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Conceptronic.ndi]
AddReg                  = USB_14B2_3C06.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Planex.ndi]
AddReg                  = USB_2019_ED06.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[D-Link.ndi]
AddReg                  = USB_07D1_3C09.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[AL.ndi]
AddReg                  = USB_14B2_3C07.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Airlink.ndi]
AddReg                  = USB_14B2_3C23.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Corega.ndi]
AddReg                  = USB_07AA_002F.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Gigabyte.ndi]
AddReg                  = USB_1044_800B.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Sparklan.ndi]
AddReg                  = USB_15A9_0006.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[SMC.ndi]
AddReg                  = USB_083A_B522.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Arcadyan.ndi]
AddReg                  = USB_083A_7522.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[ZCOM.ndi]
AddReg                  = USB_0CDE_0022.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[EnGenius.ndi]
AddReg                  = USB_1740_9701.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Philips.ndi]
AddReg                  = USB_0471_200F.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Draytek.ndi]
AddReg                  = USB_14B2_3C25.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[AzureWave.ndi]
AddReg                  = USB_13D3_3247.ndi.reg, Common.reg, USB9X.ndi.reg, RemoveFlag.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[Ralink.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Ralink_2770.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[ASUS.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[ASUSGEN.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[ASUS1742.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Sitecom.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Conceptronic.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Planex.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[D-Link.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[AL.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Airlink.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Corega.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Gigabyte.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Sparklan.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[SMC.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Arcadyan.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[ZCOM.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[EnGenius.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Philips.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Draytek.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[AzureWave.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

; NT services sections
[Ralink.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Ralink_2770.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[ASUS.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[ASUSGEN.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[ASUS1742.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Sitecom.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Conceptronic.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Planex.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[D-Link.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[AL.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Airlink.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Corega.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Gigabyte.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Sparklan.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[SMC.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Arcadyan.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[ZCOM.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[EnGenius.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Philips.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[Draytek.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[AzureWave.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Country Region G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region 11G"
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, "(Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum,    1,                  0, "(Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum,    2,                  0, "(Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum,    3,                  0, "(Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum,    4,                  0, "(Channel 14)"
HKR, NDI\params\CountryRegion\enum,    5,                  0, "(Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum,    6,                  0, "(Channel 3 - 9)"
HKR, NDI\params\CountryRegion\enum,    7,                  0, "(Channel 5 - 13)"

;
; Country Region A Band
;
HKR, ,                                 CountryRegionABand, 0, "0"
HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, "Country Region 11A"
HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
HKR, NDI\params\CountryRegionABand,    default,            0, "0"
HKR, NDI\params\CountryRegionABand\enum,0,                 0, "Ch(36 - 64,149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,1,                 0, "Ch(36 - 140)"
HKR, NDI\params\CountryRegionABand\enum,2,                 0, "Ch(36 - 64)"
HKR, NDI\params\CountryRegionABand\enum,3,                 0, "Ch(52 - 64,149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,4,                 0, "Ch(149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,5,                 0, "Ch(149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,6,                 0, "Ch(36 - 48)"
HKR, NDI\params\CountryRegionABand\enum,7,                 0, "Ch(36 - 165)"
HKR, NDI\params\CountryRegionABand\enum,8,                 0, "Ch(52 - 64)"

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "5"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "0"

;
; Enable patch for pass wifi 11n draft
;
HKR, ,                            TGnWifiTest,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"
HKR, NDI\params\BGProtection,           ParamDesc, 0, "B/G Protection"
HKR, NDI\params\BGProtection,           type,      0, "enum"
HKR, NDI\params\BGProtection,           default,   0, "0"
HKR, NDI\params\BGProtection\enum,      0,         0, "Auto"
HKR, NDI\params\BGProtection\enum,      1,         0, "On"
HKR, NDI\params\BGProtection\enum,      2,         0, "Off"

;
; FrameAggregation
;
HKR, ,                            FrameAggregation,0, "0"
HKR, NDI\params\FrameAggregation,       ParamDesc, 0, "Frame Aggregation"
HKR, NDI\params\FrameAggregation,       type,      0, "enum"
HKR, NDI\params\FrameAggregation,       default,   0, "1"
HKR, NDI\params\FrameAggregation\enum,  0,         0, "Disable"
HKR, NDI\params\FrameAggregation\enum,  1,         0, "Enable"

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, "IEEE802.11h"
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, "Disable"
HKR, NDI\params\IEEE80211H\enum,  1,               0, "Enable"

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"
HKR, NDI\params\AutoChannelSelect,       ParamDesc,0, "Auto Channel Select"
HKR, NDI\params\AutoChannelSelect,       type,     0, "enum"
HKR, NDI\params\AutoChannelSelect,       default,  0, "0"
HKR, NDI\params\AutoChannelSelect\enum,  0,        0, "Disable"
HKR, NDI\params\AutoChannelSelect\enum,  1,        0, "Enable"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, "WMM Capable"
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "0"
HKR, NDI\params\WMMCapable\enum,        0,         0, "Disable"
HKR, NDI\params\WMMCapable\enum,        1,         0, "Enable"

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"
HKR, NDI\params\APSDCapable,            ParamDesc, 0, "APSD Capable"
HKR, NDI\params\APSDCapable,            type,      0, "enum"
HKR, NDI\params\APSDCapable,            default,   0, "0"
HKR, NDI\params\APSDCapable\enum,       0,         0, "Disable"
HKR, NDI\params\APSDCapable\enum,       1,         0, "Enable"

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"
HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, "AC_BE support APSD"
HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
HKR, NDI\params\APSDAC_BE,              default,   0, "0"
HKR, NDI\params\APSDAC_BE\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BE\enum,         1,         0, "Enable"

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"
HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, "AC_BK support APSD"
HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
HKR, NDI\params\APSDAC_BK,              default,   0, "0"
HKR, NDI\params\APSDAC_BK\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BK\enum,         1,         0, "Enable"

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"
HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, "AC_VI support APSD"
HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
HKR, NDI\params\APSDAC_VI,              default,   0, "0"
HKR, NDI\params\APSDAC_VI\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VI\enum,         1,         0, "Enable"

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"
HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, "AC_VO support APSD"
HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
HKR, NDI\params\APSDAC_VO,              default,   0, "0"
HKR, NDI\params\APSDAC_VO\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VO\enum,         1,         0, "Enable"

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
HKR, Default,                     MaxSPLength,     0, "0"
HKR, NDI\params\MaxSPLength,      ParamDesc,       0, "Max Service Period Length"
HKR, NDI\params\MaxSPLength,      type,            0, "int"
HKR, NDI\params\MaxSPLength,      default,         0, "0"
HKR, NDI\params\MaxSPLength,      min,             0, "0"
HKR, NDI\params\MaxSPLength,      max,             0, "3"
HKR, NDI\params\MaxSPLength,      step,            0, "1"
HKR, NDI\params\MaxSPLength,      optional,        0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "0"
HKR, NDI\params\DLSCapable,             ParamDesc, 0, "DLS Capable"
HKR, NDI\params\DLSCapable,             type,      0, "enum"
HKR, NDI\params\DLSCapable,             default,   0, "0"
HKR, NDI\params\DLSCapable\enum,        0,         0, "Disable"
HKR, NDI\params\DLSCapable\enum,        1,         0, "Enable"

;
; RDG
;
HKR, ,                            RDG,      0, "1"
HKR, NDI\params\RDG,                    ParamDesc, 0, "RDG"
HKR, NDI\params\RDG,                    type,      0, "enum"
HKR, NDI\params\RDG,                    default,   0, "1"
HKR, NDI\params\RDG\enum,               0,         0, "Disable"
HKR, NDI\params\RDG\enum,               1,         0, "Enable"

;
; AllowBW40InBGBand
;
HKR, ,                            AllowBW40InBGBand,      0, "1"
HKR, NDI\params\AllowBW40InBGBand,      ParamDesc, 0, "AllowBW40InBGBand"
HKR, NDI\params\AllowBW40InBGBand,      type,      0, "enum"
HKR, NDI\params\AllowBW40InBGBand,      default,   0, "1"
HKR, NDI\params\AllowBW40InBGBand\enum, 0,         0, "Disable"
HKR, NDI\params\AllowBW40InBGBand\enum, 1,         0, "Enable"

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "0"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "0"
HKR, NDI\params\PSPXlink\enum,    0,               0, "Disable"
HKR, NDI\params\PSPXlink\enum,    1,               0, "Enable"

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Block ACK settings
;
HKR, ,                            BACapability,      0x10001, "0x07034020"
HKR, Default,                     BACapability,      0x10001, "0x07034020"


;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting,      0x10001, "0x2ba15"
HKR, Default,                     TransmitSetting,      0x10001, "0x2ba15"


;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
;HKR, ,                            SSID,            0, %SSID_DEF_STR%
;HKR, Default,                     SSID,            0, %SSID_DEF_STR%
;HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
;HKR, NDI\params\SSID,             type,            0, "edit"
;HKR, NDI\params\SSID,             limitText,       0, "32"
;HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "1"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "1"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

[RemoveFlag.reg]
HKR, ,                SafelyRemoveOff,    0, "1"

;*******************************************************************************************
; DeviceID for Win9X 
;*******************************************************************************************
[USB_148F_2870.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_148F&PID_2870"

[USB_148F_2770.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_148F&PID_2770"

[USB_0B05_1731.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0B05&PID_1731"

[USB_0B05_1732.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0B05&PID_1732"

[USB_0B05_1742.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0B05&PID_1742"

[USB_0DF6_0017.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0DF6&PID_0017"

[USB_14B2_3C06.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_14B2&PID_3C06"

[USB_2019_ED06.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_2019&PID_ED06"

[USB_07D1_3C09.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_07D1&PID_3C09"

[USB_14B2_3C07.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_14B2&PID_3C07"

[USB_14B2_3C23.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_14B2&PID_3C23"

[USB_07AA_002F.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_07AA&PID_002F"

[USB_1044_800B.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_1044&PID_800B"

[USB_15A9_0006.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_15A9&PID_0006"

[USB_083A_B522.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_083A&PID_B522"

[USB_083A_7522.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_083A&PID_7522"

[USB_0CDE_0022.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0CDE&PID_0022"

[USB_1740_9701.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_1740&PID_9701"

[USB_0471_200F.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_0471&PID_200F"

[USB_14B2_3C25.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_14B2&PID_3C25"

[USB_13D3_3247.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "USB\VID_13D3&PID_3247"

[USB9X.ndi.reg]
HKR, ,                            NTMPDriver,       0, rt28709x.sys

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt28709x.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt28709x"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
win9x.CopyFiles         = 11    ; system32 subdirectory on win9x

[NT.CopyFiles]
rt2870.sys                   ; NT Installation

[win9x.CopyFiles]
rt28709x.sys                     ;  Win9x Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt2870.sys              = 1
rt28709x.sys            = 1

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2870"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[Generic.Service]
DisplayName                 = %Generic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2870.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2870.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Ralink                      = "Ralink Technology, Corp."
Asus                        = "ASUSTeK Computer Inc."
Sitecom                     = "Sitecom Europe BV"
Conceptronic                = "Conceptronic"
Planex                      = "Planex Communications, Inc."
D-Link                      = "D-Link"
AL                          = "AL Tech., Inc."
Airlink                     = "Airlink"
Corega                      = "Corega"
Gigabyte                    = "Gigabyte"
Sparklan                    = "Sparklan Communications, Inc."
SMC                         = "SMC Networks, Inc."
Arcadyan                    = "Arcadyan Technology Corporation"
ZCOM                        = " "
EnGenius                    = "EnGenius Technologies"
Philips                     = "Philips"
Draytek                     = "Draytek"
AzureWave                   = "AzureWave Technologies, Inc."

Generic.DeviceDesc          = "802.11n USB Wireless LAN Card"
ASUS.DeviceDesc             = "ASUS 802.11n Network Adapter"
ASUSGEN.DeviceDesc          = "802.11n Network Adapter"
ASUS1742.DeviceDesc         = "802.11n Network Adapter"
Sitecom.DeviceDesc          = "Wireless-N Network USB Adapter WL-182"
Conceptronic.DeviceDesc     = "Wireless 300Mbps 11.N USB Adapter"
Planex.DeviceDesc           = "PCI 802.11n Wireless LAN USB Adapter"
D-Link.DeviceDesc           = "D-Link DWA-140 RangeBooster N USB Adapter"
AL.DeviceDesc               = "AnyGate 11N W-LAN Adapter (XM-242U)"
Airlink.DeviceDesc          = "Airlink101 300N Wireless USB Adapter"
Corega.DeviceDesc           = "CG-WLUSB2GNL"
Gigabyte.DeviceDesc         = "Gigabyte GN-WB30N 802.11n USB WLAN Card"
Sparklan.DeviceDesc         = "Wireless 11n USB Adapter"
SMC.DeviceDesc              = "EZ Connect N Draft 11n Wireless USB2.0 Adapter"
Arcadyan.DeviceDesc         = "802.11N Wireless USB Adapter"
ZCOM.DeviceDesc             = "802.11b/g/n USB Wireless Network Adapter"
EnGenius.DeviceDesc         = "EnGenius 802.11n Wireless USB Adapter"
Philips.DeviceDesc          = "Philips 802.11n Wireless USB Adapter"
Draytek.DeviceDesc          = "Vigor N61 802.11n Wireless USB Adapter"
AzureWave.DeviceDesc        = "802.11 n/g/b Wireless LAN USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11n Wireless Card."
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"

