;****************************************************************************************
;
; NetRT61G.inf
;
;   This installation script supports Windows Vista for the
;   D-Link RT61 series Wireless LAN Card
;
;   Copyright (c)2006,D-Link Corporation 
;   All Rights Reserved.

;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Provider%
Compatible      = 1
DriverVer       = 12/11/2006,2.00.03.0000
CatalogFile     = NetRT61G.CAT            

[ControlFlags]
ExcludeFromSelect = VEN_1814&DEV_0301&SUBSYS_3C081186
ExcludeFromSelect = VEN_1814&DEV_0301&SUBSYS_3C091186
ExcludeFromSelect = VEN_1814&DEV_0302&SUBSYS_3C081186
ExcludeFromSelect = VEN_1814&DEV_0302&SUBSYS_3C091186
ExcludeFromSelect = VEN_1814&DEV_0302&SUBSYS_3A711186
ExcludeFromSelect = VEN_1814&DEV_0302&SUBSYS_3A721186
ExcludeFromSelect = VEN_1814&DEV_0302&SUBSYS_3C101186
ExcludeFromSelect = VEN_1814&DEV_0302&SUBSYS_3C111186
ExcludeFromSelect = VEN_1814&DEV_0302&SUBSYS_3C121186
ExcludeFromSelect = VEN_1814&DEV_0302&SUBSYS_3C131186

[Manufacturer]
%Provider%        = D-Link


[D-Link]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%G630.DeviceDesc%    = NetRT61G_0302.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_3C081186
%G510.DeviceDesc%    = NetRT61G_0302.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_3C091186
%G630B.DeviceDesc%    = NetRT61G_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_3C081186
%G510B.DeviceDesc%    = NetRT61G_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_3C091186
%DWA510.DeviceDesc%    = NetRT61G_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_3A711186
%DWA610.DeviceDesc%    = NetRT61G_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_3A721186
%G650A.DeviceDesc%    = NetRT61G_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_3C101186
%G520A.DeviceDesc%    = NetRT61G_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_3C111186
%G630M.DeviceDesc%    = NetRT61G_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_3C121186
%G510M.DeviceDesc%    = NetRT61G_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_3C131186

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[NetRT61G_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles
*IfType			= 71                        ; IF_TYPE_IEEE80211
*MediaType		= 16                        ; NdisMediumNative802_11
*PhysicalMediaType	= 9                         ; NdisPhysicalMediumNative802_11

[NetRT61G_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles
*IfType			= 71                        ; IF_TYPE_IEEE80211
*MediaType		= 16                        ; NdisMediumNative802_11
*PhysicalMediaType	= 9                         ; NdisPhysicalMediumNative802_11

[NetRT61G_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles
*IfType			= 71                        ; IF_TYPE_IEEE80211
*MediaType		= 16                        ; NdisMediumNative802_11
*PhysicalMediaType	= 9                         ; NdisPhysicalMediumNative802_11

; NT services sections
[NetRT61G_0301.ndi.NT.Services]
AddService              = RT61, 2, RALINK.Service, common.EventLog

[NetRT61G_0302.ndi.NT.Services]
AddService              = RT61, 2, RALINK.Service, common.EventLog

[NetRT61G_0401.ndi.NT.Services]
AddService              = RT61, 2, RALINK.Service, common.EventLog

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

HKR, Ndi,                       Service,    0, "RT61"

HKR, Ndi\params\*ReceiveBuffers,  ParamDesc,  0, "ReceiveBuffers"
HKR, Ndi\params\*ReceiveBuffers,  default,    0, "64"
HKR, Ndi\params\*ReceiveBuffers,  min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,  max,        0, "00000128"
HKR, Ndi\params\*ReceiveBuffers,  step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,  Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,  type,       0, "int"

HKR, Ndi\params\*TransmitBuffers, ParamDesc,  0, "TransmitBuffers"
HKR, Ndi\params\*TransmitBuffers, default,    0, "64"
HKR, Ndi\params\*TransmitBuffers, min,        0, "1"
HKR, Ndi\params\*TransmitBuffers, max,        0, "00000064"
HKR, Ndi\params\*TransmitBuffers, step,       0, "1"
HKR, Ndi\params\*TransmitBuffers, Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers, type,       0, "int"

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "1"   ; 0=disable(default), 1=enable

;
; Country Region G Band
;
;HKR, ,                                 CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region 11G"
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, "(Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    1,                  0, "(Channel 1 - 13)"
;HKR, NDI\params\CountryRegion\enum,    2,                  0, "(Channel 10 - 11)"
;HKR, NDI\params\CountryRegion\enum,    3,                  0, "(Channel 10 - 13)"
;HKR, NDI\params\CountryRegion\enum,    4,                  0, "(Channel 14)"
;HKR, NDI\params\CountryRegion\enum,    5,                  0, "(Channel 1 - 14)"
;HKR, NDI\params\CountryRegion\enum,    6,                  0, "(Channel 3 - 9)"
;HKR, NDI\params\CountryRegion\enum,    7,                  0, "(Channel 5 - 13)"

;
; Country Region A Band
;
;HKR, ,                                 CountryRegionABand, 0, "7"
;HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, "Country Region 11A"
;HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
;HKR, NDI\params\CountryRegionABand,    default,            0, "7"
;HKR, NDI\params\CountryRegionABand\enum,0,                 0, "Ch(36 - 64,149 - 165)"
;HKR, NDI\params\CountryRegionABand\enum,1,                 0, "Ch(36 - 140)"
;HKR, NDI\params\CountryRegionABand\enum,2,                 0, "Ch(36 - 64)"
;HKR, NDI\params\CountryRegionABand\enum,3,                 0, "Ch(52 - 64,149 - 161)"
;HKR, NDI\params\CountryRegionABand\enum,4,                 0, "Ch(149 - 165)"
;HKR, NDI\params\CountryRegionABand\enum,5,                 0, "Ch(149 - 161)"
;HKR, NDI\params\CountryRegionABand\enum,6,                 0, "Ch(36 - 48)"
;HKR, NDI\params\CountryRegionABand\enum,7,                 0, "Ch(36 - 165)"
;HKR, NDI\params\CountryRegionABand\enum,8,                 0, "Ch(52 - 64)"
;HKR, NDI\params\CountryRegionABand\enum,9,                 0, "Ch(34 - 46)"
;HKR, NDI\params\CountryRegionABand\enum,10,                0, "Ch(34 - 64)"
;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "3"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "0"
HKR, NDI\params\AdhocOfdm,              ParamDesc, 0, "Adhoc Wireless Mode"
HKR, NDI\params\AdhocOfdm,              type,      0, "enum"
HKR, NDI\params\AdhocOfdm,              default,   0, "0"
HKR, NDI\params\AdhocOfdm\enum,         0,         0, "802.11 B Only"
HKR, NDI\params\AdhocOfdm\enum,         1,         0, "802.11 B/G Mix"
HKR, NDI\params\AdhocOfdm\enum,         2,         0, "802.11 G Only"


;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"
HKR, NDI\params\BGProtection,           ParamDesc, 0, "B/G Protection"
HKR, NDI\params\BGProtection,           type,      0, "enum"
HKR, NDI\params\BGProtection,           default,   0, "0"
HKR, NDI\params\BGProtection\enum,      0,         0, "Auto"
HKR, NDI\params\BGProtection\enum,      1,         0, "On"
HKR, NDI\params\BGProtection\enum,      2,         0, "Off"

;
; FrameAggregation
;
HKR, ,                            FrameAggregation,0, "1"
HKR, NDI\params\FrameAggregation,       ParamDesc, 0, "Frame Aggregation"
HKR, NDI\params\FrameAggregation,       type,      0, "enum"
HKR, NDI\params\FrameAggregation,       default,   0, "1"
HKR, NDI\params\FrameAggregation\enum,  0,         0, "Disable"
HKR, NDI\params\FrameAggregation\enum,  1,         0, "Enable"

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, "IEEE802.11h"
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, "Disable"
HKR, NDI\params\IEEE80211H\enum,  1,               0, "Enable"

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"
HKR, NDI\params\AutoChannelSelect,       ParamDesc,0, "Auto Channel Select"
HKR, NDI\params\AutoChannelSelect,       type,     0, "enum"
HKR, NDI\params\AutoChannelSelect,       default,  0, "0"
HKR, NDI\params\AutoChannelSelect\enum,  0,        0, "Disable"
HKR, NDI\params\AutoChannelSelect\enum,  1,        0, "Enable"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, "WMM Capable"
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "1"
HKR, NDI\params\WMMCapable\enum,        0,         0, "Disable"
HKR, NDI\params\WMMCapable\enum,        1,         0, "Enable"
;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "1"
HKR, NDI\params\APSDCapable,            ParamDesc, 0, "APSD Capable"
HKR, NDI\params\APSDCapable,            type,      0, "enum"
HKR, NDI\params\APSDCapable,            default,   0, "1"
HKR, NDI\params\APSDCapable\enum,       0,         0, "Disable"
HKR, NDI\params\APSDCapable\enum,       1,         0, "Enable"

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "1"
HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, "AC_BE support APSD"
HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
HKR, NDI\params\APSDAC_BE,              default,   0, "1"
HKR, NDI\params\APSDAC_BE\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BE\enum,         1,         0, "Enable"

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "1"
HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, "AC_BK support APSD"
HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
HKR, NDI\params\APSDAC_BK,              default,   0, "1"
HKR, NDI\params\APSDAC_BK\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BK\enum,         1,         0, "Enable"

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "1"
HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, "AC_VI support APSD"
HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
HKR, NDI\params\APSDAC_VI,              default,   0, "1"
HKR, NDI\params\APSDAC_VI\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VI\enum,         1,         0, "Enable"

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "1"
HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, "AC_VO support APSD"
HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
HKR, NDI\params\APSDAC_VO,              default,   0, "1"
HKR, NDI\params\APSDAC_VO\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VO\enum,         1,         0, "Enable"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "1"
HKR, NDI\params\DLSCapable,             ParamDesc, 0, "DLS Capable"
HKR, NDI\params\DLSCapable,             type,      0, "enum"
HKR, NDI\params\DLSCapable,             default,   0, "0"
HKR, NDI\params\DLSCapable\enum,        0,         0, "Disable"
HKR, NDI\params\DLSCapable\enum,        1,         0, "Enable"

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
HKR, ,                            SSID,            0, %SSID_DEF_STR%
HKR, Default,                     SSID,            0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
HKR, NDI\params\SSID,             type,            0, "edit"
HKR, NDI\params\SSID,             limitText,       0, "32"
HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "32"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "32"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
XP.CopyFiles            = 12    ; system32\drivers subdirectory on Windows XP
win9x.CopyFiles         = 11    ; system subdirectory on win9x

[NT.CopyFiles]
rt61.sys                        ; NT Installation

[XP.CopyFiles]
rt61.sys

[win9x.CopyFiles]
rt619x.sys                      ; Win9x Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt61.sys                = 1
rt619x.sys              = 1

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RT61.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "RT61"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "wlan,ethernet"

[RALINK.Service]
DisplayName                 = %RALINK.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT61.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[Strings]
Provider                      = "D-Link"

;*******************************************************************************************
; Device description
;*******************************************************************************************
G630.DeviceDesc      = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter(rev.E)"
G510.DeviceDesc      = "D-Link AirPlus G DWL-G510 Wireless PCI Adapter(rev.C)"
G630B.DeviceDesc      = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter(rev.E)"
G510B.DeviceDesc      = "D-Link AirPlus G DWL-G510 Wireless PCI Adapter(rev.C)"
DWA610.DeviceDesc      = "D-Link Wireless G DWA-610 Notebook Adapter"
DWA510.DeviceDesc      = "D-Link Wireless G DWA-510 Desktop Adapter"
G650A.DeviceDesc      = "D-Link AirPlus G DWL-G650+A Wireless Cardbus Adapter(rev.E)"
G520A.DeviceDesc      = "D-Link AirPlus G DWL-G520+A Wireless PCI Adapter(rev.C)"
G630M.DeviceDesc      = "D-Link AirPlus G DWL-G630M Wireless Cardbus Adapter(rev.A)"
G510M.DeviceDesc      = "D-Link AirPlus G DWL-G510M Wireless PCI Adapter(rev.A)"

INSTALL_DISK_STR            = "D-Link AirPlus G Installation Disk"
RALINK.Service.DispName     = "D-Link Wireless Driver"


; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR                = "dlink"
VENDOR_DESC_DEF_STR         = "D-Link 802.11g Wireless LAN Card."
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "6"

