[Version]
Signature="$WINDOWs NT$"
Class=Multifunction
ClassGuid={4d36e971-e325-11ce-bfc1-08002be10318}
provider=%MFGNAME%
;CatalogFile=EMV98P.cat
;DriverVer=12/10/2001,1.0.1.3
DriverVer=05/10/2004,1.0.0.0

[ControlFlags]
Excludefromselect=USB\VID_058F&PID_9520

[Manufacturer]
%MFGNAME%=DeviceList

[DestinationDirs]
DriverCopyFiles  = 10,System32\Drivers
SMCLIB.CopyFiles = 10,System32\Drivers
DefaultDestDir   = 10,System32\Drivers

[SourceDisksFiles]
EMV98P.sys=1
EMV98P.inf=1
smclib.sys=1
EMV98Lib.sys=1
EMV98ChA.sys=1
EMV98ChB.sys=1
EMV98ChC.sys=1

[SourceDisksNames]
1=%INSTDISK%,,,

[DeviceList]
%USB\VID_058F&PID_9520.DeviceDesc%=DriverInstall,USB\VID_058F&PID_9520

;------------------------------------------------------------------------------
;  Windows 98 Installation
;------------------------------------------------------------------------------
[DriverInstall]
AddReg=DriverAddReg,SMCLIB.AddReg,Class.AddReg
CopyFiles=DriverCopyFiles,SMCLIB.CopyFiles

[SMCLIB.CopyFiles]
;smclib.sys
EMV98P.sys
EMV98Lib.sys
EMV98ChA.sys
EMV98ChB.sys
EMV98ChC.sys

[DriverAddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,EMV98P.sys

[DriverInstall.hw]
AddReg=DriverHwAddReg

[SMCLIB.AddReg]
HKR,,DevLoader,,*NTKERN

[Class.AddReg]
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0000","DevLoader",,"*ntkern"
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0000","DriverDate",,"5-10-2004"       
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0000","DriverDesc",,"Au9520 SlotA"    
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0000","InfPath",," "                  
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0000","InfSection",," "               
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0000","NTMPDriver",,"emv98cha.sys"    
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0000","ProviderName",,"ALCOR EMVSCARD"

HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0001","DevLoader",,"*ntkern"
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0001","DriverDate",,"5-10-2004"       
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0001","DriverDesc",,"Au9520 SlotB"    
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0001","InfPath",," "                  
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0001","InfSection",," "               
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0001","NTMPDriver",,"emv98chb.sys"    
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0001","ProviderName",,"ALCOR EMVSCARD"

HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0002","DevLoader",,"*ntkern"
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0002","DriverDate",,"5-10-2004"       
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0002","DriverDesc",,"Au9520 SlotC"    
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0002","InfPath",," "                  
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0002","InfSection",," "               
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0002","NTMPDriver",,"emv98chc.sys"    
HKLM,"System\CurrentControlSet\Services\Class\SmartCardReader\0002","ProviderName",,"ALCOR EMVSCARD"

HKLM,"Enum\Root\*AlcorEMV9520\0000","Capabilities",1,14,00,00,00
HKLM,"Enum\Root\*AlcorEMV9520\0000","Class",,"SmartCardReader"                           
HKLM,"Enum\Root\*AlcorEMV9520\0000","ClassGUID",,"{50DD5230-BA8A-11D1-BF5D-0000F805F530}"
HKLM,"Enum\Root\*AlcorEMV9520\0000","ConfigFlags",1,00,00,00,00                       
HKLM,"Enum\Root\*AlcorEMV9520\0000","DeviceDesc",,"ALCOR EMV SC Slot A"                  
HKLM,"Enum\Root\*AlcorEMV9520\0000","Driver",,"SmartCardReader\0000"                    
HKLM,"Enum\Root\*AlcorEMV9520\0000","HardwareID",,"*SLOTA"                               
HKLM,"Enum\Root\*AlcorEMV9520\0000","Mfg",," "                                           
HKLM,"Enum\Root\*AlcorEMV9520\0000","Serial",1,04,00,00,00,00,00,00,00                

HKLM,"Enum\Root\*AlcorEMV9520\0001","Capabilities",1,14,00,00,00
HKLM,"Enum\Root\*AlcorEMV9520\0001","Class",,"SmartCardReader"                           
HKLM,"Enum\Root\*AlcorEMV9520\0001","ClassGUID",,"{50DD5230-BA8A-11D1-BF5D-0000F805F530}"
HKLM,"Enum\Root\*AlcorEMV9520\0001","ConfigFlags",1,00,00,00,00                       
HKLM,"Enum\Root\*AlcorEMV9520\0001","DeviceDesc",,"ALCOR EMV SC Slot B"                  
HKLM,"Enum\Root\*AlcorEMV9520\0001","Driver",,"SmartCardReader\0001"                    
HKLM,"Enum\Root\*AlcorEMV9520\0001","HardwareID",,"*SLOTB"                               
HKLM,"Enum\Root\*AlcorEMV9520\0001","Mfg",," "                                           
HKLM,"Enum\Root\*AlcorEMV9520\0001","Serial",1,05,00,00,00,00,00,00,00                

HKLM,"Enum\Root\*AlcorEMV9520\0002","Capabilities",1,14,00,00,00
HKLM,"Enum\Root\*AlcorEMV9520\0002","Class",,"SmartCardReader"                           
HKLM,"Enum\Root\*AlcorEMV9520\0002","ClassGUID",,"{50DD5230-BA8A-11D1-BF5D-0000F805F530}"
HKLM,"Enum\Root\*AlcorEMV9520\0002","ConfigFlags",1,00,00,00,00                       
HKLM,"Enum\Root\*AlcorEMV9520\0002","DeviceDesc",,"ALCOR EMV SC Slot C"                  
HKLM,"Enum\Root\*AlcorEMV9520\0002","Driver",,"SmartCardReader\0002"
HKLM,"Enum\Root\*AlcorEMV9520\0002","HardwareID",,"*SLOTC"                               
HKLM,"Enum\Root\*AlcorEMV9520\0002","Mfg",," "                                           
HKLM,"Enum\Root\*AlcorEMV9520\0002","Serial",1,06,00,00,00,00,00,00,00                

;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------
[Strings]
MFGNAME="EMVSCARD"
USB\VID_058F&PID_9520.DeviceDesc="Au9520 EMV Certified USB Smart Card Reader"
INSTDISK="Installation Disc for Au9520 USB Reader"
