;+--------------------------------------------------------------------------+
;| Device name    : ZyXEL G-320H IEEE 802.11g Wireless High Power PCI Adapter|
;| Platform	  : Microsoft Windows 2000 / XP / XP64                      |
;| Host interface : PCI                                                     |
;|                                                                          |
;| Copyright (c) 2000-2004 ZyXEL Technology Corporation.                    |
;| All Rights Reserved.                                                     |
;+--------------------------------------------------------------------------+

;-------------------------------------------------------------------------
[Version]
Signature		= "$Chicago$"
Compatible		= 1
Class			= Net
ClassGUID		= {4d36e972-e325-11ce-bfc1-08002be10318}
MillenniumPreferred	= .ME
Provider		= %INFProvider%
;CatalogFile		= zd1212Bp.cat			; for WHQL certified
CatalogFile.NT		= G320H.cat			; for WHQL certified
DriverVer		= 07/20/2006,1.5.4.6


[Manufacturer]
%Manufacturer%	= ZyXEL, NT.5.1, ntamd64


[ControlFlags]


[ZyXEL]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------
%ZD1212B_50U_DESC%       = ZD1212B_50U.ndi,   PCI\VEN_167B&DEV_2116&SUBSYS_187E3410&REV_01


[ZyXEL.NT.5.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------
%ZD1212B_50U_DESC%       = ZD1212BXP_50U, PCI\VEN_167B&DEV_2116&SUBSYS_187E3410&REV_01

[ZyXEL.ntamd64]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------
%ZD1212B_50U_DESC%       = ZD1212BXP_50U.ntamd64, PCI\VEN_167B&DEV_2116&SUBSYS_187E3410&REV_01

;*********************************************************************
;   Microsoft Windows 98 section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1212B_50U.ndi]
AddReg		= ZD1212B_Win9x.reg, ZD1212B_Common.reg, UnZDRegistryPCI.reg
CopyFiles       = ZD1212B.CopyFiles98
DriverVer	= 07/20/2006,1.5.4.6



[ZD1212B_Win9x.reg]
HKR,NDI,              DeviceID,           0, %ZD1212B_50U_PNP%
HKR,NDI,              CardType,           0, %CardType%
HKR,,                 DevLoader,          0, "*ndis"
HKR,,                 DeviceVxDs,         0, %DriverFileName%

; NDIS Info
HKR,NDIS,             MajorNdisVersion,   1, 03
HKR,NDIS,             MinorNdisVersion,   1, 0A
HKR,NDIS,             LogDriverName,      0, %CustomServiceName%(%Manufacturer%)

; Interfaces Info
HKR,NDI\Interfaces,   DefUpper,           0, "ndis3"
HKR,NDI\Interfaces,   DefLower,           0, "ethernet"
HKR,NDI\Interfaces,   UpperRange,         0, "ndis3"
HKR,NDI\Interfaces,   LowerRange,         0, "ethernet"

; Other Info
HKR,,                 BusType,            0, 15
HKR,,                 IOBaseAddress,      1, 02,00,00,00
HKR,,                 InterruptNumber,    1, 04,00,00,00
HKR,,                 EnumPropPages,      0, "netdi.dll,EnumPropPages"

; Install Sections
HKR,NDI\Install,      ndis3,              0, "ZD1212B.ndis3"

HKR,,                 VendorDesc,         0, %VendorDesc%


[ZD1212B.CopyFiles98]
G320H.sys,G320H98.sys,,2

;*********************************************************************
;   Microsoft Windows Me section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1212B_50U.ndi.ME]
Characteristics = 0x84
BusType         = 15
AddReg		= ZD1212B_WinMe.reg, ZD1212B_Common.reg, UnZDRegistryPCI.reg
CopyFiles       = ZD1212B.CopyFilesMe


[ZD1212B_50U.ndi.ME.Services]
AddService = %CustomServiceName%(%Manufacturer%), 2, ZD1212BP_ME.Service, ZD1212BP.EventLog


[ZD1212B_WinMe.reg]
HKR,NDI,              Service,            0, %CustomServiceName%(%Manufacturer%)
HKR,,                 DevLoader,          0, "*ndis"
HKR,,                 DeviceVxDs,         0, %DriverFileName%
HKR,,                 EnumPropPages,      0, "netdi.dll,EnumPropPages"

; NDIS Info
HKR,NDIS,             MajorNdisVersion,   1, 05
HKR,NDIS,             MinorNdisVersion,   1, 00
HKR,NDIS,             LogDriverName,      0, %CustomServiceName%(%Manufacturer%)

; Interfaces Info
HKR,NDI\Interfaces,   DefUpper,           0, "ndis5"
HKR,NDI\Interfaces,   DefLower,           0, "ethernet"
HKR,NDI\Interfaces,   UpperRange,         0, "ndis5"
HKR,NDI\Interfaces,   LowerRange,         0, "ethernet"

; Install Sections
HKR,NDI\Install,      ndis3,              0, "ZD1212B.ndis5me"

HKR,,                 VendorDesc,         0, %VendorDesc%


[ZD1212B.ndis5me]
CopyFiles       = ZD1212B.CopyFilesMe


[ZD1212B.CopyFilesMe]
G320H.sys,G320HME.sys,,2


[ZD1212BP_ME.Service]
DisplayName     = %ZD1212BP.Service.DispName%(%Manufacturer%)
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %11%\%DriverFileName%		; %11%\zd1212BP.sys
LoadOrderGroup  = NDIS


;*********************************************************************
;   Microsoft Windows 2000 section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1212B_50U.ndi.NTx86]
Characteristics = 0x84
BusType         = 15
AddReg		= ZD1212B_Win2K.reg, ZD1212B_Common.reg
CopyFiles       = ZD1212B.CopyFiles2K

[ZD1212B_50U.ndi.NTx86.Services]
AddService = %CustomServiceName%(%Manufacturer%), 2, ZD1212BP_NT.Service, ZD1212BP.EventLog

[ZD1212B_Win2K.reg]
; Interfaces Info
HKR,NDI\Interfaces,   UpperRange,         0, "ndis5"
HKR,NDI\Interfaces,   LowerRange,         0, "ethernet"
HKR,NDI,              Service,            0, %CustomServiceName%(%Manufacturer%)

HKR,,                 VendorDesc,         0, %VendorDesc%


[ZD1212B.CopyFiles2K]
G320H.sys,G320H2K.sys,,2

;*********************************************************************
;   Microsoft Windows XP section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1212BXP_50U.NTx86]
Characteristics = 0x84
BusType         = 15
AddReg		= ZD1212B_WinXP.reg, ZD1212B_Common.reg
CopyFiles       = ZD1212B.CopyFilesXP


[ZD1212BXP_50U.NTx86.Services]
AddService = %CustomServiceName%(%Manufacturer%), 2, ZD1212BP_NT.Service, ZD1212BP.EventLog

[ZD1212BXP_50U.ntamd64]
Characteristics = 0x84
BusType         = 15
AddReg		= ZD1212B_WinXP.reg, ZD1212B_Common.reg
CopyFiles       = ZD1212B.CopyFilesXP64

[ZD1212BXP_50U.ntamd64.Services]
AddService = %CustomServiceName%(%Manufacturer%), 2, ZD1212BP_NT.Service, ZD1212BP.EventLog

[ZD1212B_WinXP.reg]
; Interfaces Info
HKR,NDI\Interfaces,   UpperRange,         0, "ndis5"
HKR,NDI\Interfaces,   LowerRange,         0, "ethernet"
HKR,NDI,              Service,            0, %CustomServiceName%(%Manufacturer%)
HKR,,                 VendorDesc,         0, %VendorDesc%


[ZD1212B.CopyFilesXP]
G320H.sys,G320HXP.sys,,2

[ZD1212B.CopyFilesXP64]
G320H.sys,G320H64.sys,,2
;*********************************************************************
;   Microsoft Windows 2000/XP Common Section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1212BP_NT.Service]
DisplayName     = %ZD1212BP.Service.DispName%(%Manufacturer%)
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\%DriverFileName%		; %12%\%DriverFileName%
LoadOrderGroup  = NDIS


;*********************************************************************
;   Microsoft Windows ME/2000/XP Common Section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1212BP.EventLog]
Addreg = ZD1212BP.AddEventLog.reg

[ZD1212BP.AddEventLog.reg]
HKR,,                               EventMessageFile,  0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,,                               TypesSupported,    0x00010001, 7


;*********************************************************************
;   Destination Directories
;*********************************************************************
[DestinationDirs]
ZD1212B.CopyFiles98	= 11			; system subdirectory on Win 98
ZD1212B.CopyFilesMe	= 11			; system subdirectory on Win Me
ZD1212B.CopyFiles2K	= 12			; system32\drivers subdirectory on Win NT/2000
ZD1212B.CopyFilesXP	= 12			; system32\drivers subdirectory on Win XP
ZD1212B.CopyFilesXP64	= 12			; system32\drivers subdirectory on Win XP64


[SourceDisksNames]
1=%DISKNAME%,,,


[SourceDisksFiles]
G320H98.sys = 1
G320HME.sys = 1
G320H2K.sys = 1
G320HXP.sys = 1
G320H64.sys = 1


;******************************************************************************
[ZD1212B_Common.reg]
HKR, Ndi\params\NumRfd,         ParamDesc,  	0, "%ReceiveFrameDescriptors%"
HKR, Ndi\params\NumRfd,         default,    	0, "32"
HKR, Ndi\params\NumRfd,         min,        	0, "1"
HKR, Ndi\params\NumRfd,         max,        	0, "00001024"
HKR, Ndi\params\NumRfd,         step,       	0, "1"
HKR, Ndi\params\NumRfd,         Base,       	0, "10"
HKR, Ndi\params\NumRfd,         type,       	0, "int"
HKR, Ndi\params\NumRfd,         flag, 		1, 20,00,00,00

HKR, Ndi\params\NumTcb,         ParamDesc,  	0, "%TransmitControlBlocks%"
HKR, Ndi\params\NumTcb,         default,    	0, "32"
HKR, Ndi\params\NumTcb,         min,        	0, "1"
HKR, Ndi\params\NumTcb,         max,        	0, "00000064"
HKR, Ndi\params\NumTcb,         step,       	0, "1"
HKR, Ndi\params\NumTcb,         Base,       	0, "10"
HKR, Ndi\params\NumTcb,         type,		0, "int"
HKR, Ndi\params\NumTcb,         flag,		1, 20,00,00,00

HKR, Ndi\params\NumCoalesce,    ParamDesc,  	0, "%CoalesceBuffers%"
HKR, Ndi\params\NumCoalesce,    default,    	0, "128"
HKR, Ndi\params\NumCoalesce,    min,        	0, "1"
HKR, Ndi\params\NumCoalesce,    max,        	0, "00000128"
HKR, Ndi\params\NumCoalesce,    step,       	0, "1"
HKR, Ndi\params\NumCoalesce,    Base,       	0, "10"
HKR, Ndi\params\NumCoalesce,    type,       	0, "int"
HKR, Ndi\params\NumCoalesce,    flag, 		1, 20,00,00,00

HKR,,                           	PreambleMode,   0, "0"
HKR,NDI\params\PreambleMode,    	ParamDesc,      0, "PreambleMode"
HKR,NDI\params\PreambleMode,       	type,           0, "enum"
HKR,NDI\params\PreambleMode,           	flag,           1, 30,00,00,00
HKR,Ndi\params\PreambleMode,           	default,        0, "3"
HKR,NDI\params\PreambleMode\enum,      	1,              0, "Long"
HKR,NDI\params\PreambleMode\enum,      	2,              0, "Short"
HKR,NDI\params\PreambleMode\enum,      	3,              0, "Auto"

;HKR,,                           	IBSS_G_Mode,    0, "0"
;HKR,NDI\params\IBSS_G_Mode,    	        ParamDesc,      0, "IBSS_G_Mode"
;HKR,NDI\params\IBSS_G_Mode,       	type,           0, "enum"
;HKR,NDI\params\IBSS_G_Mode,           	flag,           1, 30,00,00,00
;HKR,Ndi\params\IBSS_G_Mode,           	default,        0, "0"
;HKR,NDI\params\IBSS_G_Mode\enum,      	0,              0, "Disable"
;HKR,NDI\params\IBSS_G_Mode\enum,      	1,              0, "Enable"

;HKR,,                           	IBSS_PureG_Mode,0, "0"
;HKR,NDI\params\IBSS_PureG_Mode,    	ParamDesc,      0, "IBSS_PureG_Mode"
;HKR,NDI\params\IBSS_PureG_Mode,       	type,           0, "enum"
;HKR,NDI\params\IBSS_PureG_Mode,         flag,           1, 30,00,00,00
;HKR,Ndi\params\IBSS_PureG_Mode,         default,        0, "0"
;HKR,NDI\params\IBSS_PureG_Mode\enum,    0,              0, "Disable"
;HKR,NDI\params\IBSS_PureG_Mode\enum,    1,              0, "Enable"

HKR,,                           		IBSS Wireless Mode,   0, "0"
HKR,NDI\params\IBSS Wireless Mode,    		ParamDesc,      0, "IBSS Wireless Mode"
HKR,NDI\params\IBSS Wireless Mode,       	type,           0, "enum"
HKR,NDI\params\IBSS Wireless Mode,           	flag,           1, 30,00,00,00
HKR,Ndi\params\IBSS Wireless Mode,           	default,        0, "0"
HKR,NDI\params\IBSS Wireless Mode\enum,      	0,              0, "IBSS B Mode"
HKR,NDI\params\IBSS Wireless Mode\enum,      	1,              0, "IBSS G Mode"

HKR,,                           	IBSS Protection Mode,0, "0"
HKR,NDI\params\IBSS Protection Mode,    	ParamDesc,      0, "IBSS Protection Mode"
HKR,NDI\params\IBSS Protection Mode,       	type,           0, "enum"
HKR,NDI\params\IBSS Protection Mode,         flag,           1, 30,00,00,00
HKR,Ndi\params\IBSS Protection Mode,         default,        0, "0"
HKR,NDI\params\IBSS Protection Mode\enum,    0,              0, "Disable"
HKR,NDI\params\IBSS Protection Mode\enum,    1,              0, "Enable"

HKR,,                           	TxBurst_Mode,   0, "0"
HKR,NDI\params\TxBurst_Mode,    	ParamDesc,      0, "TxBurst_Mode"
HKR,NDI\params\TxBurst_Mode,       	type,           0, "enum"
HKR,NDI\params\TxBurst_Mode,            flag,           1, 30,00,00,00
HKR,Ndi\params\TxBurst_Mode,            default,        0, "0"
HKR,NDI\params\TxBurst_Mode\enum,       0,              0, "Disable"
HKR,NDI\params\TxBurst_Mode\enum,       5,              0, "Enable"

HKR,,                           	PSPXLinkMode,   0, "0"
HKR,NDI\params\PSPXLinkMode,    	        ParamDesc,      0, "PSPXLinkMode"
HKR,NDI\params\PSPXLinkMode,       	type,           0, "enum"
HKR,NDI\params\PSPXLinkMode,           	flag,           1, 30,00,00,00
HKR,Ndi\params\PSPXLinkMode,           	default,        0, "0"
HKR,NDI\params\PSPXLinkMode\enum,      	0,              0, "Disable"
HKR,NDI\params\PSPXLinkMode\enum,      	1,              0, "Enable"

HKR,,                            QosTagPolicy,   0, "0"
HKR,NDI\params\QosTagPolicy,     ParamDesc,      0, "QosTagPolicy"
HKR,NDI\params\QosTagPolicy,        type,           0, "enum"
HKR,NDI\params\QosTagPolicy,            flag,           1, 30,00,00,00
HKR,Ndi\params\QosTagPolicy,            default,        0, "0"
HKR,NDI\params\QosTagPolicy\enum,       0,              0, "Auto"
HKR,NDI\params\QosTagPolicy\enum,       1,              0, "802.1Q Tag"
HKR,NDI\params\QosTagPolicy\enum,       2,              0, "DSCP Tag"

HKR,,                            WMMQosSupport,   0, "0"
HKR,NDI\params\WMMQosSupport,             ParamDesc,      0, "WMMQosSupport"
HKR,NDI\params\WMMQosSupport,        type,           0, "enum"
HKR,NDI\params\WMMQosSupport,            flag,           1, 30,00,00,00
HKR,Ndi\params\WMMQosSupport,            default,        0, "0"
HKR,NDI\params\WMMQosSupport\enum,       0,              0, "Disable"
HKR,NDI\params\WMMQosSupport\enum,       1,              0, "Enable"

HKR,NDI\params\Active Radar Detect,         ParamDesc,      0, "Active Radar Detect"
HKR,NDI\params\Active Radar Detect,         type,           0, "enum"
HKR,NDI\params\Active Radar Detect,         flag,           1, 30,00,00,00
HKR,Ndi\params\Active Radar Detect,         default,        0, "0"
HKR,NDI\params\Active Radar Detect\enum,    0,              0, "Disable"
HKR,NDI\params\Active Radar Detect\enum,    1,              0, "Enable"

HKR,,                           A_Band_6M_36M_Equal_Power, 0, "1"
HKR,,                           PHY_A_6M_Setpoint_Value,	0x10001, 0x28
HKR,,                           PHY_A_6M_CR128_Value,	0x10001, 0x17
HKR,,                           PHY_A_1dBm_Value,	0x10001, 0x10
HKR,,                           EnableAntennaDiversity, 0, "0"
HKR,,                           DefaultAntenna, 0, "0"
HKR,,                           DefaultWirelessMode, 0, "0"
HKR,,                           SaveDefaultConnection, 0, "1"
HKR,,                           Active Radar Detect,0, "0"
HKR,,                           ZDIBSSOpenAAllowChannel, 0, "0"




;*********************************************************************
[UnZDRegistryPCI.reg]
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\UNZD1212B%InterfaceType%,DEL_HKR_0000,0,"ENUM\"%ZD1212B_50U_PNP%


;*********************************************************************
[Strings]
INFProvider	= "ZyXEL"
Manufacturer	= "ZyXEL"

DISKNAME	= "ZyXEL G-320H IEEE 802.11g Wireless LAN Driver (PCI) Installation Disk"

DriverFileName	= "G320H.sys"
InterfaceType	= "PCI"
CardType	= "PNP"
VendorDesc	= "ZyXEL G-320H 802.11g Wireless LAN"
CustomServiceName = "G320H"

ZD1212B_50U_DESC	= "ZyXEL G-320H IEEE 802.11g Wireless PCI Adapter"
ZD1212B_50U_PNP  = "PCI\VEN_167B&DEV_2116&SUBSYS_187E3410&REV_01"

ReceiveFrameDescriptors = "ReceiveFrameDescriptors"
TransmitControlBlocks = "TransmitControlBlocks"
CoalesceBuffers = "CoalesceBuffers"

ZD1212BP.Service.DispName = "ZyXEL G-320H IEEE 802.11g Wireless LAN Driver (PCI)"
